# reprap-prusa-i3-documents
by Jannik Beyerstedt from Hamburg, Germany  
[jannikbeyerstedt.de](http://jannikbeyerstedt.de) | [Github](https://github.com/jbeyerstedt)  
**license:** CC-BY-SA-4.0

## my "private" settings
These are the settings and tests I use for my reprap prusa i3 build.

## configuration

- prusa i3 sheet model
  - wodden sheets, watercut. reenfoced at the top by some piece of wood
  - simple selfmade wooden filament spool holder at the top
  - all metric standards
  - T2.5 belts
- electronics
  - RAMPS 1.4
  - mkII headbed
  - NEMA17 stepper motors
  - 200W 12V power supply by meanwell
- extruder/ hotend
  - 3mm filament
  - J-Head
  - Greg´s Wade Extruder
  - Layer fan
- OctoPrint on Rapberry Pi 2B


## location of settings files

#### OS X:
- Slic3r: ~/Library/Application Support/Slic3r
- printrun: ~/.pronsolerc

##### Windows:
- Slic3r: 
- printrun:

